**Fanvil X7 Enterprise IP Phone**

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Highlights*** Virtual programmable keypad - 4 pages can be dynamically displayed, and 29 DSS keys can be set on each page. Up to 127 DSS keys can be customized.Each DSS key can be set to Line/BLF/ speed dial etc.
* Gigabit Ethernet – 10/100/1000Mbps Ethernet with POE enabled.
* Economic and Environmental Friendly design with Elegant

Housing, with high-resolution TFT color display, delivering a rich visual experience.* High Interoperability – Compatible with major platforms: 3CX, Asterisk, Broadsoft, Elastix, Zycoo, etc.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Model** | **Screen** | **Network** | **POE** | **Power adapter** |
| **X7** | **7.0” color-screen** | **10/100/1000Mbps** | **√** | **×** |

 | **x7-03(181122)** |

The Fanvil X7 IP Phone is a high-end enterprise phone with 7-inch touch screen, which greatly improves the efficiency of the enterprise with advanced design and high cost performance.

**Generic**

* 20 SIP Lines
* HD Voice
* Support receiving Video call­­­­­­­­
* POE Enabled
* 7 Inch Electric Capacity Touch Screen
* Handset / Hands-free / Headset mode
* Intelligent DSS Keys
* Optional External Power Supply

**Call Features**

* Call out / Answer / Reject
* Mute / Unmute (microphone)
* Call Hold / Resume
* Call Waiting
* Intercom
* Caller ID Display
* Speed Dial
* Anonymous Call (Hide Caller ID)
* Call Forwarding (Always/Busy/No Answer)
* Call Transfer (Attended/Unattended)
* Call Parking/Pick-up (depending on server)
* Redial
* Do-Not-Disturb
* Auto-Answering
* Voice Message (on server)
* 3-way Conference
* Hot Line
* Hot desking

**Phone Features**

* Local Phonebook (2000 entries)
* Remote Phonebook (XML/LDAP, 2000 entries)
* Call logs (in/out/missed, 1000 entries)
* Black/White List Call Filtering
* Screen saver
* Voice Message Waiting Indication (VMWI)
* Programmable DSS/Soft keys
* Network Time Synchronization
* Built-in Bluetooth 2.1: Support Bluetooth headset
* Support Wi-Fi Dongle
* Support Plantronics wireless headset (Through Plantronics APD-80 EHS Cable)
* Support Jabra wireless headset (Through Fanvil EHS20 EHS Cable)
* Support Recording (Through Flash Drive or Server Recording )
* Action URL / Active URI
* uaCSTA

**Video**

* Video codec: H.264
* Video call resolution: QCIF / CIF / VGA

**Audio**

* HD Voice Microphone/Speaker (Handset/Hands-free, 0 ~ 7KHz Frequency Response)
* HAC handset
* Wideband ADC/DAC 16KHz Sampling
* Narrowband CODEC: G.711a/u, G.723.1, G.726-32K, G.729AB, AMR, iLBC
* Wideband CODEC: G.722, AMR-WB, Opus
* Full-duplex Acoustic Echo Canceller (AEC)
* Voice Activity Detection (VAD) / Comfort Noise Generation (CNG) / Background Noise Estimation (BNE) / Noise Reduction (NR)
* Packet Loss Concealment (PLC)
* Dynamic Adaptive Jitter Buffer up to 300ms
* DTMF: In-band, Out-of-Band – DTMF-Relay(RFC2833) / SIP INFO

**Networking**

* Physical: 10/100/1000 Mbps Ethernet, dual bridged port for PC bypass
* IP Mode:IPv4/IPv6/IPv4&IPv6
* IP Configuration: Static / DHCP / PPPoE
* Network Access Control: 802.1x
* VPN: L2TP / OpenVPN
* VLAN
* LLDP
* QoS
* RTCP-XR(RFC3611),VQ-RTCPXR(RFC6035)

**Protocols**

* SIP2.0 over UDP/TCP/TLS
* RTP/RTCP/SRTP
* STUN
* DHCP
* IPv6
* LLDP
* PPPoE
* 802.1x
* L2TP
* OpenVPN
* SNTP
* FTP/TFTP
* HTTP/HTTPS
* TR-069

**Deployment & Maintenance**

* Auto-Provisioning via FTP/TFTP/HTTP/HTTPS/DHCP OPT66/SIP PNP/TR-069
* Web Management Portal
* Web-based Packet Dump
* Configuration Export / Import
* Phonebook Import/Export
* Firmware Upgrade
* Syslog

**Physical Specifications**

* Main LCD x1: 7.0 inch (800x480) Capacitive touch screen
* Keypad: 26 keys, including
* 5 Function keys (Hold, MWI,Mute,Headset, Redial)
* 4 Navigation keys
* 1 OK key
* 1 Return key
* 12 Standard Phone Digits keys
* 2 Volume Control keys, Up/Down
* 1 Hands-free key
* HD Handset (RJ9) x1
* Standard RJ9 Handset Wire x1
* 1.5M CAT5 Ethernet Cable x1
* Back Rack x1
* RJ9 Port x2: Handset x1, Headset x1
* RJ45 Port x2: Network x1, PC x1 (Bridged to Network)
* USB2.0 Port x1: Standard A, Connect with Wi-Fi USB dongle or Flash Driver
* DC Power Input: 5V/2A
* Power Consumption (POE): 2.6~9W
* Power Consumption (Adapter): 2.4~8W
* Working Temperature: 0~40℃
* Working Humidity: 10~95%
* Installation: Desktop Stand
* Color: Black
* Device Dimensions
* Desktop Stand (angles 1): 268x185x189mm
* Desktop Stand (angles 2): 268x201x168mm
* Gift Box Dimensions: 342x271x63mm
* Outer CTN Dimensions: 570x340x365mm (10 PCS)

The above specifications may be updated in the future without prior notice. All hardware/software/physical features should be based on the final shipped products. Customers should consult Fanvil’s retailers, distributors, or Fanvil directly, if customers have concerns on any feature.

For more information, please visit: [www.fanvil.com](http://www.fanvil.com)

**Compatibility List:**

